# Name: AKSHAY SING JJ Ex. No.: 9 Roll no:231901005

**INSTALL AND CONFIGURE IPTABLES FIREWALL**

**Aim:**

To install iptables and configure it for variety of options.

**Common Configurations & outputs:**

# 1. Start/stop/restart firewalls

[root@localhost ~]# systemctl start firewalld

[root@localhost ~]# systemctl restart firewalld

[root@localhost ~]# systemctl stop firewalld

[root@localhost ~]#

# 2. Check all exitsting IPtables Firewall Rules

[root@localhost ~]# iptables -L -n -v

[root@localhost ~]#

# 3. Block specific IP Address(eg. 172.16.8.10) in IPtables Firewall

[root@localhost ~]# iptables -A INPUT -s 172.16.8.10 -j DROP

[root@localhost ~]#

# 4. Block specifig port on IPtables Firewall

[root@localhost ~]# iptables -A OUTPUT -p tcp --dport xxx -j DROP

[root@localhost ~]#

# 5. Allow specific network range on particular port on iptables

[root@localhost ~]# iptables -A OUTPUT -p tcp -d 172.16.8.0/24 --dport xxx -j ACCEPT [root@localhost ~]#

6. **Block Facebook on IPTables** [root@localhost ~]# host facebook.com facebook.com has address 157.240.24.35

facebook.com has IPv6 address 2a03:2880:f10c:283:face:b00c:0:25de facebook.com mail is handled by 10 smtpin.vvv.facebook.com.

[root@localhost ~]# whois 157.240.24.35 | grep CIDR

CIDR: 157.240.0.0/16

[root@localhost ~]#

[root@localhost ~]# whois 157.240.24.35

[Querying whois.arin.net]

[whois.arin.net]

#

# ARIN WHOIS data and services are subject to the Terms of Use

# available at: https://www.arin.net/resources/registry/whois/tou/ #

# If you see inaccuracies in the results, please report at

# https://www.arin.net/resources/registry/whois/inaccuracy\_reporting/

#

# Copyright 1997-2019, American Registry for Internet Numbers, Ltd.

#

NetRange: 157.240.0.0 - 157.240.255.255

CIDR: 157.240.0.0/16

NetName: THEFA-3

NetHandle: NET-157-240-0-0-1

Parent: NET157 (NET-157-0-0-0-0) NetType: Direct Assignment OriginAS:

Organization: Facebook, Inc. (THEFA-3)

RegDate: 2015-05-14

Updated: 2015-05-14

Ref: https://rdap.arin.net/registry/ip/157.240.0.0

OrgName: Facebook, Inc. OrgId: THEFA-3 Address: 1601 Willow Rd.

City: Menlo Park

StateProv: CA

PostalCode: 94025

Country: US

RegDate: 2004-08-11

Updated: 2012-04-17

Ref: https://rdap.arin.net/registry/entity/THEFA-3

OrgTechHandle: OPERA82-ARIN

OrgTechName: Operations

OrgTechPhone: +1-650-543-4800

OrgTechEmail: domain@facebook.com

OrgTechRef: https://rdap.arin.net/registry/entity/OPERA82-ARIN

OrgAbuseHandle: OPERA82-ARIN

OrgAbuseName: Operations

OrgAbusePhone: +1-650-543-4800

OrgAbuseEmail: domain@facebook.com

OrgAbuseRef: https://rdap.arin.net/registry/entity/OPERA82-ARIN

#

# ARIN WHOIS data and services are subject to the Terms of Use

# available at: https://www.arin.net/resources/registry/whois/tou/

#

# If you see inaccuracies in the results, please report at

# https://www.arin.net/resources/registry/whois/inaccuracy\_reporting/ #

# Copyright 1997-2019, American Registry for Internet Numbers, Ltd. #

[root@localhost ~]# iptables -A OUTPUT -p tcp -d 157.240.0.0/16 -j DROP Open browser and check whether http://facebook.com is accessible

To allow facebook use -D instead of -A option

[root@localhost ~]# iptables -D OUTPUT -p tcp -d 157.240.0.0/16 -j DROP [root@localhost ~]#

# 6. Block Access to your system from specific MAC Address(say 0F:22:1E:00:02:30)

[root@localhost ~]# iptables -A INPUT -m mac --mac-source 0F:22:1E:00:02:30 -j DROP [root@localhost ~]#

# 7.Save IPtables rules to a file

[root@localhost ~]# iptables-save > ~/iptables.rules

[root@localhost ~]# vi iptables.rules

[root@localhost ~]#

# 8.Restrict number of concurrent connections to a Server(Here restrict to 3 connections only)

[root@localhost ~]# iptables -A INPUT -p tcp --syn --dport 22 -m connlimit --connlimitabove 3 -j REJECT

# 9. Disable outgoing mails through IPtables

[root@localhost ~]# iptables -A OUTPUT -p tcp --dport 25 -j REJECT

[root@localhost ~]#

# 10. Flush IPtables Firewall chains or rules

[root@localhost ~]# iptables -F

[root@localhost ~]#

**Result:**

Thus, the iptables has been installed successfully and it has been configured for variety of options.